IFC building model
Schema: "IFC4"
Description: "ViewDefinition [Ifc4NotAssigned]"
File name: "C:\Autodesk\mounting edge view point.ifc"
Time stamp: "2024-07-22T11:37:27"
Author: "info"
Organization: "MDC Software Solutions LLC"
Preprocessor: "IFCout / IFCout Cloud version 2024.07.07"
Originating system: "IFCoutCommon"
Authorization: "None"
Application: "GeometryGymIFCcore v24.5.8.0" version "v24.5.8.0" identifier "GeometryGymIFCcore v24.5.8.0" by Organization "Geometry Gym Pty Ltd"

People and organizations
  Person id "info" of Organization "LAPTOP-J4V1U9U2"
  Organization "MDC Software Solutions LLC"
  Owner history of Person id "info" of Organization "LAPTOP-J4V1U9U2" | application "GeometryGymIFCcore v24.5.8.0" version "v24.5.8.0" identifier "GeometryGymIFCcore v24.5.8.0" by Organization "Geometry Gym Pty Ltd" | change ADDED | created 1721666245 (2024-07-22T16:37:25Z) | last modified 1721666245 (2024-07-22T16:37:25Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "mounting edge view point"
  IFCBUILDING "mounting edge view point" | postal address: "Unknown", "Unknown", "Unknown", "Unknown"
    contains 1911 elements
      714 x IFCBEAM | BEAM | names: "CHS114.3x5", "RD12", "RHS60x40x3" (+167 more) | property sets: BEAM
      402 x IFCMECHANICALFASTENER | BOLT | names: "20ø XOX" | property sets: BOLT
      671 x IFCPLATE | object type "PLATE" | names: "PL 10x6-15/16"x180", "PL 10x6-7/8"x180", "PL 10x2-3/4"x232.2" (+493 more) | property sets: PLATE
      112 x IFCBEAM | SPANDREL | property sets: BENTBEAM
      10 x IFCMECHANICALFASTENER | ANCHORBOLT | property sets: ANCHORBOLT
      1 x IFCSLAB | FLOOR | property sets: SLAB
      1 x IFCFOOTING | PAD_FOOTING | property sets: ISOLATEDFOOTING

Property sets
  BEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "CHS114.3x5" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "153,76,0" (IFCLABEL)
    Exact weight = "30.939224187826905" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2189901963840)" (IFCLABEL)
    Insertion line from X = "12380.856024260975" (IFCLABEL)
    Insertion line from Y = "8985.747453626056" (IFCLABEL)
    Insertion line from Z = "-872.0036661873085" (IFCLABEL)
    Insertion line to X = "13428.02121070914" (IFCLABEL)
    Insertion line to Y = "6811.336735791828" (IFCLABEL)
    Insertion line to Z = "-871.9376533895404" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Painting area = "836880.897330609" (IFCLABEL)
    PnPClassName = "ASTBEAM" (IFCLABEL)
    Real length = "2330.598977941335" (IFCLABEL)
    Section = "O" (IFCLABEL)
    Section Class = "UK Circular Hollow Section" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "2413.424310372934" (IFCLABEL)
    Weight = "13.47751102371655" (IFCLABEL)
  BEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "CHS114.3x5" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "153,76,0" (IFCLABEL)
    Exact weight = "27.70935998206462" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2189901963824)" (IFCLABEL)
    Insertion line from X = "11765.067496662232" (IFCLABEL)
    Insertion line from Y = "8689.205104614892" (IFCLABEL)
    Insertion line from Z = "-456.23074195977597" (IFCLABEL)
    Insertion line to X = "12812.232683110396" (IFCLABEL)
    Insertion line to Y = "6514.7943867806625" (IFCLABEL)
    Insertion line to Z = "-456.1647291620079" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Painting area = "750271.5361408995" (IFCLABEL)
    PnPClassName = "ASTBEAM" (IFCLABEL)
    Real length = "2089.403738197266" (IFCLABEL)
    Section = "O" (IFCLABEL)
    Section Class = "UK Circular Hollow Section" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "2413.424310372934" (IFCLABEL)
    Weight = "13.47751102371655" (IFCLABEL)
  BEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "CHS114.3x5" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "153,76,0" (IFCLABEL)
    Exact weight = "24.479495776295604" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2189901963808)" (IFCLABEL)
    Insertion line from X = "11149.278969063489" (IFCLABEL)
    Insertion line from Y = "8392.662755603726" (IFCLABEL)
    Insertion line from Z = "-40.457817732244166" (IFCLABEL)
    Insertion line to X = "12196.444155511654" (IFCLABEL)
    Insertion line to Y = "6218.252037769496" (IFCLABEL)
    Insertion line to Z = "-40.39180493447611" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Painting area = "663662.1749511939" (IFCLABEL)
    PnPClassName = "ASTBEAM" (IFCLABEL)
    Real length = "1848.208498453206" (IFCLABEL)
    Section = "O" (IFCLABEL)
    Section Class = "UK Circular Hollow Section" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "2413.424310372934" (IFCLABEL)
    Weight = "13.47751102371655" (IFCLABEL)
  BEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "CHS114.3x5" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "153,76,0" (IFCLABEL)
    Exact weight = "21.24963157053076" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2189901963792)" (IFCLABEL)
    Insertion line from X = "10533.490441464746" (IFCLABEL)
    Insertion line from Y = "8096.120406592561" (IFCLABEL)
    Insertion line from Z = "375.31510649528764" (IFCLABEL)
    Insertion line to X = "11580.65562791291" (IFCLABEL)
    Insertion line to Y = "5921.709688758333" (IFCLABEL)
    Insertion line to Z = "375.3811192930557" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Painting area = "577052.8137614836" (IFCLABEL)
    PnPClassName = "ASTBEAM" (IFCLABEL)
    Real length = "1607.0132587091346" (IFCLABEL)
    Section = "O" (IFCLABEL)
    Section Class = "UK Circular Hollow Section" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "2413.424310372933" (IFCLABEL)
    Weight = "13.47751102371655" (IFCLABEL)
  BEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "CHS114.3x5" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "153,76,0" (IFCLABEL)
    Exact weight = "18.019767364769216" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2189901963776)" (IFCLABEL)
    Insertion line from X = "9917.701913866003" (IFCLABEL)
    Insertion line from Y = "7799.578057581398" (IFCLABEL)
    Insertion line from Z = "791.0880307228203" (IFCLABEL)
    Insertion line to X = "10964.867100314168" (IFCLABEL)
    Insertion line to Y = "5625.1673397471695" (IFCLABEL)
    Insertion line to Z = "791.1540435205884" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Painting area = "490443.4525717762" (IFCLABEL)
    PnPClassName = "ASTBEAM" (IFCLABEL)
    Real length = "1365.8180189650689" (IFCLABEL)
    Section = "O" (IFCLABEL)
    Section Class = "UK Circular Hollow Section" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "2413.424310372933" (IFCLABEL)
    Weight = "13.47751102371655" (IFCLABEL)
  BEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "CHS114.3x5" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "153,76,0" (IFCLABEL)
    Exact weight = "14.789903159006915" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2189901963760)" (IFCLABEL)
    Insertion line from X = "9301.91338626726" (IFCLABEL)
    Insertion line from Y = "7503.035708570234" (IFCLABEL)
    Insertion line from Z = "1206.8609549503533" (IFCLABEL)
    Insertion line to X = "10349.078572715425" (IFCLABEL)
    Insertion line to Y = "5328.624990736006" (IFCLABEL)
    Insertion line to Z = "1206.9269677481213" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Painting area = "403834.09138206777" (IFCLABEL)
    PnPClassName = "ASTBEAM" (IFCLABEL)
    Real length = "1124.622779221" (IFCLABEL)
    Section = "O" (IFCLABEL)
    Section Class = "UK Circular Hollow Section" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "2413.4243103729336" (IFCLABEL)
    Weight = "13.47751102371655" (IFCLABEL)
  BEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "CHS114.3x5" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "153,76,0" (IFCLABEL)
    Exact weight = "11.56003895323812" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2189901963744)" (IFCLABEL)
    Insertion line from X = "8686.124858668516" (IFCLABEL)
    Insertion line from Y = "7206.493359559067" (IFCLABEL)
    Insertion line from Z = "1622.633879177886" (IFCLABEL)
    Insertion line to X = "9733.29004511668" (IFCLABEL)
    Insertion line to Y = "5032.082641724839" (IFCLABEL)
    Insertion line to Z = "1622.699891975654" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Painting area = "317224.73019235814" (IFCLABEL)
    PnPClassName = "ASTBEAM" (IFCLABEL)
    Real length = "883.4275394769306" (IFCLABEL)
    Section = "O" (IFCLABEL)
    Section Class = "UK Circular Hollow Section" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "2413.4243103729336" (IFCLABEL)
    Weight = "13.47751102371655" (IFCLABEL)
  BEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "CHS114.3x5" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "153,76,0" (IFCLABEL)
    Exact weight = "30.939224187830234" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2189901988992)" (IFCLABEL)
    Insertion line from X = "13407.465765148307" (IFCLABEL)
    Insertion line from Y = "6883.837750830923" (IFCLABEL)
    Insertion line from Z = "-872.0036661873085" (IFCLABEL)
    Insertion line to X = "13647.786898235014" (IFCLABEL)
    Insertion line to Y = "4482.408457569656" (IFCLABEL)
    Insertion line to Z = "-871.9376533895404" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Painting area = "836880.8973306086" (IFCLABEL)
    PnPClassName = "ASTBEAM" (IFCLABEL)
    Real length = "2330.598977941336" (IFCLABEL)
    Section = "O" (IFCLABEL)
    Section Class = "UK Circular Hollow Section" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "2413.4243103729336" (IFCLABEL)
    Weight = "13.47751102371655" (IFCLABEL)
  BEAM: 706 more contents on 706 objects not shown
  BOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Assembly mark = "Not defined" (IFCLABEL)
    Bolt type = "XOX" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Handle = "3CBD9" (IFCLABEL)
    Name = "20ø XOX" (IFCLABEL)
    PnPClassName = "ASTBOLT2POINTS" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  BOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Assembly mark = "Not defined" (IFCLABEL)
    Bolt type = "XOX" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Handle = "3CBCE" (IFCLABEL)
    Name = "20ø XOX" (IFCLABEL)
    PnPClassName = "ASTBOLT2POINTS" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  BOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Assembly mark = "Not defined" (IFCLABEL)
    Bolt type = "XOX" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Handle = "3CBA5" (IFCLABEL)
    Name = "20ø XOX" (IFCLABEL)
    PnPClassName = "ASTBOLT2POINTS" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  BOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Assembly mark = "Not defined" (IFCLABEL)
    Bolt type = "XOX" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Handle = "3CB9A" (IFCLABEL)
    Name = "20ø XOX" (IFCLABEL)
    PnPClassName = "ASTBOLT2POINTS" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  BOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Assembly mark = "Not defined" (IFCLABEL)
    Bolt type = "XOX" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Handle = "3CB71" (IFCLABEL)
    Name = "20ø XOX" (IFCLABEL)
    PnPClassName = "ASTBOLT2POINTS" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  BOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Assembly mark = "Not defined" (IFCLABEL)
    Bolt type = "XOX" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Handle = "3CB66" (IFCLABEL)
    Name = "20ø XOX" (IFCLABEL)
    PnPClassName = "ASTBOLT2POINTS" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  BOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Assembly mark = "Not defined" (IFCLABEL)
    Bolt type = "XOX" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Handle = "3CB3A" (IFCLABEL)
    Name = "20ø XOX" (IFCLABEL)
    PnPClassName = "ASTBOLT2POINTS" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  BOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Assembly mark = "Not defined" (IFCLABEL)
    Bolt type = "XOX" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Handle = "3CB2F" (IFCLABEL)
    Name = "20ø XOX" (IFCLABEL)
    PnPClassName = "ASTBOLT2POINTS" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  BOLT: 394 more contents on 394 objects not shown
  PLATE | properties | on 1 object (1 IFCPLATE)
    Coating = "S275JR" (IFCLABEL)
    Color = "255,191,0" (IFCLABEL)
    Exact weight = "2486.0744879078898" (IFCLABEL)
    HOLES: All holes = "4" (IFCLABEL)
    HOLES: Bolt Holes = "245800" (IFCLABEL)
    Handle = "3CBCC" (IFCLABEL)
    ID = "Endplate" (IFCLABEL)
    Length = "0" (IFCLABEL)
    Material = "10" (IFCLABEL)
    Model Role = "711.8859855495953" (IFCLABEL)
    Name = "PL 10x6-15/16"x180" (IFCLABEL)
    Painting area = "2.4860744879078895" (IFCLABEL)
    Perimeter = "70458.33725442308" (IFCLABEL)
    PnPClassName = "ASTPLATE" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    Thickness = "175.94299277479783" (IFCLABEL)
    Weight = "CAS [Coating as specified]" (IFCLABEL)
    Width = "180.0000000000009" (IFCLABEL)
  PLATE | properties | on 1 object (1 IFCPLATE)
    Coating = "S275JR" (IFCLABEL)
    Color = "255,191,0" (IFCLABEL)
    Exact weight = "2486.074487907901" (IFCLABEL)
    HOLES: All holes = "4" (IFCLABEL)
    HOLES: Bolt Holes = "245864" (IFCLABEL)
    Handle = "3CB98" (IFCLABEL)
    ID = "Endplate" (IFCLABEL)
    Length = "0" (IFCLABEL)
    Material = "10" (IFCLABEL)
    Model Role = "711.8859855495962" (IFCLABEL)
    Name = "PL 10x6-15/16"x180" (IFCLABEL)
    Painting area = "2.486074487907901" (IFCLABEL)
    Perimeter = "70458.33725442339" (IFCLABEL)
    PnPClassName = "ASTPLATE" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    Thickness = "175.94299277479828" (IFCLABEL)
    Weight = "CAS [Coating as specified]" (IFCLABEL)
    Width = "180.00000000000063" (IFCLABEL)
  PLATE | properties | on 1 object (1 IFCPLATE)
    Coating = "S275JR" (IFCLABEL)
    Color = "255,191,0" (IFCLABEL)
    Exact weight = "2486.0744879078597" (IFCLABEL)
    HOLES: All holes = "4" (IFCLABEL)
    HOLES: Bolt Holes = "245928" (IFCLABEL)
    Handle = "3CB64" (IFCLABEL)
    ID = "Endplate" (IFCLABEL)
    Length = "0" (IFCLABEL)
    Material = "10" (IFCLABEL)
    Model Role = "711.8859855495905" (IFCLABEL)
    Name = "PL 10x6-15/16"x180" (IFCLABEL)
    Painting area = "2.48607448790786" (IFCLABEL)
    Perimeter = "70458.33725442227" (IFCLABEL)
    PnPClassName = "ASTPLATE" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    Thickness = "175.9429927747965" (IFCLABEL)
    Weight = "CAS [Coating as specified]" (IFCLABEL)
    Width = "179.9999999999993" (IFCLABEL)
  PLATE | properties | on 1 object (1 IFCPLATE)
    Coating = "S275JR" (IFCLABEL)
    Color = "255,191,0" (IFCLABEL)
    Exact weight = "2486.0744879078934" (IFCLABEL)
    HOLES: All holes = "4" (IFCLABEL)
    HOLES: Bolt Holes = "246056" (IFCLABEL)
    Handle = "3CB2D" (IFCLABEL)
    ID = "Endplate" (IFCLABEL)
    Length = "0" (IFCLABEL)
    Material = "10" (IFCLABEL)
    Model Role = "711.8859855495962" (IFCLABEL)
    Name = "PL 10x6-15/16"x180" (IFCLABEL)
    Painting area = "2.4860744879078935" (IFCLABEL)
    Perimeter = "70458.3372544232" (IFCLABEL)
    PnPClassName = "ASTPLATE" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    Thickness = "175.94299277479874" (IFCLABEL)
    Weight = "CAS [Coating as specified]" (IFCLABEL)
    Width = "180.00000000000043" (IFCLABEL)
  PLATE | properties | on 1 object (1 IFCPLATE)
    Coating = "S275JR" (IFCLABEL)
    Color = "255,191,0" (IFCLABEL)
    Exact weight = "2476.429485675995" (IFCLABEL)
    HOLES: All holes = "4" (IFCLABEL)
    HOLES: Bolt Holes = "247280" (IFCLABEL)
    Handle = "3CAF9" (IFCLABEL)
    ID = "Endplate" (IFCLABEL)
    Length = "0" (IFCLABEL)
    Material = "10" (IFCLABEL)
    Model Role = "710.520804766594" (IFCLABEL)
    Name = "PL 10x6-7/8"x180" (IFCLABEL)
    Painting area = "2.476429485675995" (IFCLABEL)
    Perimeter = "70198.95290565307" (IFCLABEL)
    PnPClassName = "ASTPLATE" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    Thickness = "175.2604023832964" (IFCLABEL)
    Weight = "CAS [Coating as specified]" (IFCLABEL)
    Width = "180.00000000000134" (IFCLABEL)
  PLATE | properties | on 1 object (1 IFCPLATE)
    Coating = "S275JR" (IFCLABEL)
    Color = "255,191,0" (IFCLABEL)
    Exact weight = "1268.0889999999981" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "202498" (IFCLABEL)
    Handle = "3CAD8" (IFCLABEL)
    ID = "Stiffener" (IFCLABEL)
    Length = "0" (IFCLABEL)
    Material = "10" (IFCLABEL)
    Model Role = "592.684271247459" (IFCLABEL)
    Name = "PL 10x2-3/4"x232.2" (IFCLABEL)
    Painting area = "1.268088999999998" (IFCLABEL)
    Perimeter = "38234.84271247455" (IFCLABEL)
    PnPClassName = "ASTPLATE" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    Thickness = "70" (IFCLABEL)
    Weight = "CAS [Coating as specified]" (IFCLABEL)
    Width = "232.19999999999968" (IFCLABEL)
  PLATE | properties | on 1 object (1 IFCPLATE)
    Coating = "S275JR" (IFCLABEL)
    Color = "255,191,0" (IFCLABEL)
    Exact weight = "1268.0889999999988" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "202504" (IFCLABEL)
    Handle = "3CABD" (IFCLABEL)
    ID = "Stiffener" (IFCLABEL)
    Length = "0" (IFCLABEL)
    Material = "10" (IFCLABEL)
    Model Role = "592.6842712474587" (IFCLABEL)
    Name = "PL 10x2-3/4"x232.2" (IFCLABEL)
    Painting area = "1.268088999999999" (IFCLABEL)
    Perimeter = "38234.842712474565" (IFCLABEL)
    PnPClassName = "ASTPLATE" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    Thickness = "70" (IFCLABEL)
    Weight = "CAS [Coating as specified]" (IFCLABEL)
    Width = "232.19999999999857" (IFCLABEL)
  PLATE | properties | on 1 object (1 IFCPLATE)
    Coating = "S275JR" (IFCLABEL)
    Color = "255,191,0" (IFCLABEL)
    Exact weight = "1268.0889999999915" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "202510" (IFCLABEL)
    Handle = "3CAA2" (IFCLABEL)
    ID = "Stiffener" (IFCLABEL)
    Length = "0" (IFCLABEL)
    Material = "10" (IFCLABEL)
    Model Role = "592.6842712474597" (IFCLABEL)
    Name = "PL 10x2-3/4"x232.2" (IFCLABEL)
    Painting area = "1.2680889999999916" (IFCLABEL)
    Perimeter = "38234.84271247439" (IFCLABEL)
    PnPClassName = "ASTPLATE" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    Thickness = "70.00000000000003" (IFCLABEL)
    Weight = "CAS [Coating as specified]" (IFCLABEL)
    Width = "232.1999999999993" (IFCLABEL)
  PLATE: 663 more contents on 663 objects not shown
  BENTBEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "FL40X10" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "255,255,127" (IFCLABEL)
    Exact weight = "0.5651391496360592" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2190090819120)" (IFCLABEL)
    Insertion line from X = "13144.239173173344" (IFCLABEL)
    Insertion line from Y = "9143.746617631095" (IFCLABEL)
    Insertion line from Z = "965.7" (IFCLABEL)
    Insertion line to X = "13031.451434442442" (IFCLABEL)
    Insertion line to Y = "9308.902681742617" (IFCLABEL)
    Insertion line to Z = "965.7" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "Railing_Kneerail_Landing#1025" (IFCLABEL)
    Painting area = "18053.510708453214" (IFCLABEL)
    PnPClassName = "ASTBENTBEAM" (IFCLABEL)
    Real length = "180.53510708453211" (IFCLABEL)
    Section = "F" (IFCLABEL)
    Section Class = "Flat" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "200.0000000000112" (IFCLABEL)
    Weight = "3.1399999999999997" (IFCLABEL)
  BENTBEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "FL40X10" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "255,255,127" (IFCLABEL)
    Exact weight = "2.8850284587416493" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2190090819088)" (IFCLABEL)
    Insertion line from X = "13621.544506921247" (IFCLABEL)
    Insertion line from Y = "8312.850969472769" (IFCLABEL)
    Insertion line from Z = "965.7" (IFCLABEL)
    Insertion line to X = "13144.239173173351" (IFCLABEL)
    Insertion line to Y = "9143.746617631085" (IFCLABEL)
    Insertion line to Z = "965.7" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "Railing_Kneerail_Landing#1024" (IFCLABEL)
    Painting area = "92146.3500790105" (IFCLABEL)
    PnPClassName = "ASTBENTBEAM" (IFCLABEL)
    Real length = "921.463500790105" (IFCLABEL)
    Section = "F" (IFCLABEL)
    Section Class = "Flat" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "958.8929538794085" (IFCLABEL)
    Weight = "3.1399999999999997" (IFCLABEL)
  BENTBEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "FL40X10" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "255,255,127" (IFCLABEL)
    Exact weight = "2.885028458741669" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2190090819056)" (IFCLABEL)
    Insertion line from X = "13988.29344322985" (IFCLABEL)
    Insertion line from Y = "7427.58085393224" (IFCLABEL)
    Insertion line from Z = "965.7" (IFCLABEL)
    Insertion line to X = "13621.544506921247" (IFCLABEL)
    Insertion line to Y = "8312.850969472769" (IFCLABEL)
    Insertion line to Z = "965.7" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "Railing_Kneerail_Landing#1023" (IFCLABEL)
    Painting area = "92146.35007900957" (IFCLABEL)
    PnPClassName = "ASTBENTBEAM" (IFCLABEL)
    Real length = "921.4635007900957" (IFCLABEL)
    Section = "F" (IFCLABEL)
    Section Class = "Flat" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "958.892953879417" (IFCLABEL)
    Weight = "3.1399999999999997" (IFCLABEL)
  BENTBEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "FL40X10" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "255,255,127" (IFCLABEL)
    Exact weight = "2.8850284587416395" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2190090819024)" (IFCLABEL)
    Insertion line from X = "14238.423094093989" (IFCLABEL)
    Insertion line from Y = "6502.571060734772" (IFCLABEL)
    Insertion line from Z = "965.7" (IFCLABEL)
    Insertion line to X = "13988.29344322985" (IFCLABEL)
    Insertion line to Y = "7427.580853932241" (IFCLABEL)
    Insertion line to Z = "965.7" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "Railing_Kneerail_Landing#1022" (IFCLABEL)
    Painting area = "92146.35007901007" (IFCLABEL)
    PnPClassName = "ASTBENTBEAM" (IFCLABEL)
    Real length = "921.4635007901006" (IFCLABEL)
    Section = "F" (IFCLABEL)
    Section Class = "Flat" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "958.8929538794198" (IFCLABEL)
    Weight = "3.1399999999999997" (IFCLABEL)
  BENTBEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "FL40X10" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "255,255,127" (IFCLABEL)
    Exact weight = "2.8850284587415125" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2190090818992)" (IFCLABEL)
    Insertion line from X = "14367.798456218967" (IFCLABEL)
    Insertion line from Y = "5553.113333699139" (IFCLABEL)
    Insertion line from Z = "965.7" (IFCLABEL)
    Insertion line to X = "14238.423094093989" (IFCLABEL)
    Insertion line to Y = "6502.5710607347755" (IFCLABEL)
    Insertion line to Z = "965.7" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "Railing_Kneerail_Landing#1021" (IFCLABEL)
    Painting area = "92146.35007900941" (IFCLABEL)
    PnPClassName = "ASTBENTBEAM" (IFCLABEL)
    Real length = "921.463500790094" (IFCLABEL)
    Section = "F" (IFCLABEL)
    Section Class = "Flat" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "958.8929538794229" (IFCLABEL)
    Weight = "3.1399999999999997" (IFCLABEL)
  BENTBEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "FL40X10" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "255,255,127" (IFCLABEL)
    Exact weight = "2.8850284587415373" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2190090818960)" (IFCLABEL)
    Insertion line from X = "14374.280768579094" (IFCLABEL)
    Insertion line from Y = "4594.9035761934565" (IFCLABEL)
    Insertion line from Z = "965.7" (IFCLABEL)
    Insertion line to X = "14367.798456218967" (IFCLABEL)
    Insertion line to Y = "5553.113333699146" (IFCLABEL)
    Insertion line to Z = "965.7" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "Railing_Kneerail_Landing#1020" (IFCLABEL)
    Painting area = "92146.35007900826" (IFCLABEL)
    PnPClassName = "ASTBENTBEAM" (IFCLABEL)
    Real length = "921.4635007900825" (IFCLABEL)
    Section = "F" (IFCLABEL)
    Section Class = "Flat" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "958.8929538794233" (IFCLABEL)
    Weight = "3.1399999999999997" (IFCLABEL)
  BENTBEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "FL40X10" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "255,255,127" (IFCLABEL)
    Exact weight = "2.8850284587415227" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2190090818928)" (IFCLABEL)
    Insertion line from X = "14257.762869217064" (IFCLABEL)
    Insertion line from Y = "3643.7823752516942" (IFCLABEL)
    Insertion line from Z = "965.7" (IFCLABEL)
    Insertion line to X = "14374.280768579094" (IFCLABEL)
    Insertion line to Y = "4594.903576193454" (IFCLABEL)
    Insertion line to Z = "965.7" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "Railing_Kneerail_Landing#1019" (IFCLABEL)
    Painting area = "92146.3500790096" (IFCLABEL)
    PnPClassName = "ASTBENTBEAM" (IFCLABEL)
    Real length = "921.4635007900961" (IFCLABEL)
    Section = "F" (IFCLABEL)
    Section Class = "Flat" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "958.8929538794164" (IFCLABEL)
    Weight = "3.1399999999999997" (IFCLABEL)
  BENTBEAM | properties | on 1 object (1 IFCBEAM)
    BOM: Name = "FL40X10" (IFCLABEL)
    Coating = "CAS [Coating as specified]" (IFCLABEL)
    Color = "255,255,127" (IFCLABEL)
    Exact weight = "2.885028458741532" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "-1" (IFCLABEL)
    ID = "(2190090818896)" (IFCLABEL)
    Insertion line from X = "14020.170966785423" (IFCLABEL)
    Insertion line from Y = "2715.473133860899" (IFCLABEL)
    Insertion line from Z = "965.7" (IFCLABEL)
    Insertion line to X = "14257.762869217064" (IFCLABEL)
    Insertion line to Y = "3643.7823752516965" (IFCLABEL)
    Insertion line to Z = "965.7" (IFCLABEL)
    Material = "S275JR" (IFCLABEL)
    Model Role = "Railing_Kneerail_Landing#1018" (IFCLABEL)
    Painting area = "92146.3500790098" (IFCLABEL)
    PnPClassName = "ASTBENTBEAM" (IFCLABEL)
    Real length = "921.463500790098" (IFCLABEL)
    Section = "F" (IFCLABEL)
    Section Class = "Flat" (IFCLABEL)
    Shrink (draw) = "0" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    System length = "958.8929538794223" (IFCLABEL)
    Weight = "3.1399999999999997" (IFCLABEL)
  BENTBEAM: 104 more contents on 104 objects not shown
  ANCHORBOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Anchor assembly = "MuS" (IFCLABEL)
    Anchor diameter = "20" (IFCLABEL)
    Anchor length = "761.6846597634701" (IFCLABEL)
    Anchor type = "kHeaded" (IFCLABEL)
    Anchor unfolded length = "300" (IFCLABEL)
    Assembly mark = "Not defined" (IFCLABEL)
    Coating = "BZP [Bright Zinc Plated]" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Drilled hole tolerance = "2" (IFCLABEL)
    Grip length = "127.5" (IFCLABEL)
    Handle = "3446F" (IFCLABEL)
    Material = "4.6" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Name = "20ø HOLDING DOWN BOLTS" (IFCLABEL)
    PnPClassName = "ASTANCHOR" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  ANCHORBOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Anchor assembly = "MuS" (IFCLABEL)
    Anchor diameter = "20" (IFCLABEL)
    Anchor length = "761.6846597634701" (IFCLABEL)
    Anchor type = "kHeaded" (IFCLABEL)
    Anchor unfolded length = "300" (IFCLABEL)
    Assembly mark = "Not defined" (IFCLABEL)
    Coating = "BZP [Bright Zinc Plated]" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Drilled hole tolerance = "2" (IFCLABEL)
    Grip length = "127.5" (IFCLABEL)
    Handle = "33E91" (IFCLABEL)
    Material = "4.6" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Name = "20ø HOLDING DOWN BOLTS" (IFCLABEL)
    PnPClassName = "ASTANCHOR" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  ANCHORBOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Anchor assembly = "MuS" (IFCLABEL)
    Anchor diameter = "20" (IFCLABEL)
    Anchor length = "761.6846597634701" (IFCLABEL)
    Anchor type = "kHeaded" (IFCLABEL)
    Anchor unfolded length = "300" (IFCLABEL)
    Assembly mark = "Not defined" (IFCLABEL)
    Coating = "BZP [Bright Zinc Plated]" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Drilled hole tolerance = "2" (IFCLABEL)
    Grip length = "127.5" (IFCLABEL)
    Handle = "338B3" (IFCLABEL)
    Material = "4.6" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Name = "20ø HOLDING DOWN BOLTS" (IFCLABEL)
    PnPClassName = "ASTANCHOR" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  ANCHORBOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Anchor assembly = "MuS" (IFCLABEL)
    Anchor diameter = "20" (IFCLABEL)
    Anchor length = "761.6846597634701" (IFCLABEL)
    Anchor type = "kHeaded" (IFCLABEL)
    Anchor unfolded length = "300" (IFCLABEL)
    Assembly mark = "Not defined" (IFCLABEL)
    Coating = "BZP [Bright Zinc Plated]" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Drilled hole tolerance = "2" (IFCLABEL)
    Grip length = "127.5" (IFCLABEL)
    Handle = "332DC" (IFCLABEL)
    Material = "4.6" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Name = "20ø HOLDING DOWN BOLTS" (IFCLABEL)
    PnPClassName = "ASTANCHOR" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  ANCHORBOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Anchor assembly = "MuS" (IFCLABEL)
    Anchor diameter = "20" (IFCLABEL)
    Anchor length = "761.6846597634701" (IFCLABEL)
    Anchor type = "kHeaded" (IFCLABEL)
    Anchor unfolded length = "300" (IFCLABEL)
    Assembly mark = "Not defined" (IFCLABEL)
    Coating = "BZP [Bright Zinc Plated]" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Drilled hole tolerance = "2" (IFCLABEL)
    Grip length = "127.5" (IFCLABEL)
    Handle = "32D05" (IFCLABEL)
    Material = "4.6" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Name = "20ø HOLDING DOWN BOLTS" (IFCLABEL)
    PnPClassName = "ASTANCHOR" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  ANCHORBOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Anchor assembly = "MuS" (IFCLABEL)
    Anchor diameter = "20" (IFCLABEL)
    Anchor length = "761.6846597634701" (IFCLABEL)
    Anchor type = "kHeaded" (IFCLABEL)
    Anchor unfolded length = "300" (IFCLABEL)
    Assembly mark = "Not defined" (IFCLABEL)
    Coating = "BZP [Bright Zinc Plated]" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Drilled hole tolerance = "2" (IFCLABEL)
    Grip length = "127.5" (IFCLABEL)
    Handle = "3272E" (IFCLABEL)
    Material = "4.6" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Name = "20ø HOLDING DOWN BOLTS" (IFCLABEL)
    PnPClassName = "ASTANCHOR" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  ANCHORBOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Anchor assembly = "MuS" (IFCLABEL)
    Anchor diameter = "20" (IFCLABEL)
    Anchor length = "761.6846597634701" (IFCLABEL)
    Anchor type = "kHeaded" (IFCLABEL)
    Anchor unfolded length = "300" (IFCLABEL)
    Assembly mark = "Not defined" (IFCLABEL)
    Coating = "BZP [Bright Zinc Plated]" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Drilled hole tolerance = "2" (IFCLABEL)
    Grip length = "127.5" (IFCLABEL)
    Handle = "32157" (IFCLABEL)
    Material = "4.6" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Name = "20ø HOLDING DOWN BOLTS" (IFCLABEL)
    PnPClassName = "ASTANCHOR" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  ANCHORBOLT | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Anchor assembly = "MuS" (IFCLABEL)
    Anchor diameter = "20" (IFCLABEL)
    Anchor length = "761.6846597634701" (IFCLABEL)
    Anchor type = "kHeaded" (IFCLABEL)
    Anchor unfolded length = "300" (IFCLABEL)
    Assembly mark = "Not defined" (IFCLABEL)
    Coating = "BZP [Bright Zinc Plated]" (IFCLABEL)
    Color = "0,255,255" (IFCLABEL)
    Drilled hole tolerance = "2" (IFCLABEL)
    Grip length = "127.5" (IFCLABEL)
    Handle = "31B79" (IFCLABEL)
    Material = "4.6" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Name = "20ø HOLDING DOWN BOLTS" (IFCLABEL)
    PnPClassName = "ASTANCHOR" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
  ANCHORBOLT: 2 more contents on 2 objects not shown
  SLAB | properties | on 1 object (1 IFCSLAB)
    BOM: Name = "0" (IFCLABEL)
    Coating = "- [None]" (IFCLABEL)
    Color = "132,132,132" (IFCLABEL)
    Exact weight = "4004.8602470993187" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "0" (IFCLABEL)
    Handle = "25D57" (IFCLABEL)
    ID = "154967" (IFCLABEL)
    Length = "2370.4520174283307" (IFCLABEL)
    Material = "C25/30" (IFCLABEL)
    Model Role = "-" (IFCLABEL)
    Name = "S600x1372.95" (IFCLABEL)
    Painting area = "9240006.799493346" (IFCLABEL)
    Perimeter = "6500.321894490426" (IFCLABEL)
    PnPClassName = "ASTSLAB" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    Thickness = "600" (IFCLABEL)
    Weight = "4004860.2470993185" (IFCLABEL)
    Width = "1372.947366762443" (IFCLABEL)
  ISOLATEDFOOTING | properties | on 1 object (1 IFCFOOTING)
    BOM: Name = "0" (IFCLABEL)
    Coating = "- [None]" (IFCLABEL)
    Color = "132,132,132" (IFCLABEL)
    Exact weight = "22610.384330074292" (IFCLABEL)
    HOLES: All holes = "0" (IFCLABEL)
    HOLES: Bolt Holes = "0" (IFCLABEL)
    Handle = "25D52" (IFCLABEL)
    ID = "154962" (IFCLABEL)
    Length = "1200" (IFCLABEL)
    Material = "C25/30" (IFCLABEL)
    Model Role = "Foundation" (IFCLABEL)
    Name = "F2000x2400" (IFCLABEL)
    Painting area = "24122284.536507037" (IFCLABEL)
    Perimeter = "7539.06540223866" (IFCLABEL)
    PnPClassName = "ASTISOLATEDFOOTING" (IFCLABEL)
    Single part mark = "Not defined" (IFCLABEL)
    Thickness = "2000" (IFCLABEL)
    Weight = "22610384.33007429" (IFCLABEL)
    Width = "1200" (IFCLABEL)